{

 "board": "duetwifi10",

 "firmware": 2.05,

 "nvram": true,

 "auto\_save": {

 "enabled": true,

 "save\_threshold": 10,

 "resume\_threshold": 11,

 "gcodes\_to\_run": "M913 X0 Y0 G91 M83 G1 Z3 E-5 F1000"

 },

 "display": {

 "type": 1,

 "encoder\_steps": 4,

 "spi\_frequency": 2000000,

 "menus": [

 {

 "name": "main",

 "value": "text C10 R20 \"Powered by Duet3D\""

 }

 ],

 "images": []

 },

 "geometry": {

 "type": "cartesian",

 "mins": [

 0,

 0,

 0

 ],

 "maxes": [

 235,

 235,

 310

 ],

 "delta\_radius": 105.6,

 "homed\_height": 250,

 "low\_dive\_height": false,

 "max\_carriage\_travel": 260,

 "print\_radius": 85,

 "rod\_length": 215,

 "z\_min": 0

 },

 "drives": [

 {

 "direction": 0,

 "microstepping": 16,

 "microstepping\_interpolation": true,

 "steps\_per\_mm": 80,

 "instant\_dv": 15,

 "max\_speed": 100,

 "acceleration": 500,

 "current": 800,

 "driver": 0,

 "endstop\_type": 1,

 "endstop\_location": 1,

 "driver\_v3": "0.0",

 "endstop\_pin": "xstop"

 },

 {

 "direction": 0,

 "microstepping": 16,

 "microstepping\_interpolation": true,

 "steps\_per\_mm": 80,

 "instant\_dv": 15,

 "max\_speed": 100,

 "acceleration": 500,

 "current": 800,

 "driver": 1,

 "endstop\_type": 1,

 "endstop\_location": 1,

 "driver\_v3": "0.1",

 "endstop\_pin": "ystop"

 },

 {

 "direction": 1,

 "microstepping": 16,

 "microstepping\_interpolation": true,

 "steps\_per\_mm": 400,

 "instant\_dv": 0.4,

 "max\_speed": 3,

 "acceleration": 100,

 "current": 800,

 "driver": 2,

 "endstop\_type": 0,

 "endstop\_location": 1,

 "endstop": null,

 "driver\_v3": "0.2",

 "endstop\_pin": "zstop"

 },

 {

 "direction": 0,

 "microstepping": 16,

 "microstepping\_interpolation": true,

 "steps\_per\_mm": 420,

 "instant\_dv": 5,

 "max\_speed": 20,

 "acceleration": 5000,

 "current": 800,

 "driver": 3,

 "driver\_v3": "0.3"

 }

 ],

 "idle": {

 "used": true,

 "factor": 50,

 "timeout": 30

 },

 "homing\_speed\_fast": 50,

 "homing\_speed\_slow": 4,

 "travel\_speed": 100,

 "z\_dive\_height": 5,

 "slow\_homing": false,

 "probe": {

 "type": "noprobe",

 "recovery\_time": 0.4,

 "trigger\_height": 2.5,

 "trigger\_value": 500,

 "x\_offset": 0,

 "y\_offset": 0,

 "speed": 2,

 "deploy": false,

 "points": [],

 "pwm\_channel": "64",

 "pwm\_inverted": false,

 "pwm\_pin": null,

 "input\_pin": "zprobe.in",

 "modulation\_pin": null

 },

 "bed\_is\_nozzle": false,

 "bed": {

 "present": true,

 "heater": 0,

 "use\_pid": false

 },

 "chamber": {

 "present": false,

 "heater": 2,

 "use\_pid": false

 },

 "heaters": [

 {

 "temp\_limit": 150,

 "scale\_factor": 100,

 "series": 4700,

 "thermistor": 100000,

 "beta": 4092,

 "c": 0,

 "channel": 0,

 "sensor": 0,

 "output\_pin": "bedheat",

 "sensor\_type": "thermistor",

 "sensor\_pin": "bedtemp"

 },

 {

 "temp\_limit": 350,

 "scale\_factor": 100,

 "series": 4700,

 "thermistor": 100000,

 "beta": 4092,

 "c": 0,

 "channel": 150,

 "sensor": 1,

 "output\_pin": "e0heat",

 "sensor\_type": "thermistor",

 "sensor\_pin": "e0temp"

 }

 ],

 "num\_nozzles": 1,

 "toolchange\_wait\_for\_temperatures": true,

 "generate\_t\_code": false,

 "tools": [

 {

 "mix\_ratio": [],

 "number": 0,

 "name": "",

 "extruders": [

 0

 ],

 "heaters": [

 1

 ],

 "fans": [

 0

 ],

 "x\_offset": 0,

 "y\_offset": 0,

 "z\_offset": 0

 }

 ],

 "compensation\_x\_offset": 15,

 "compensation\_y\_offset": 15,

 "peripheral\_points": 3,

 "halfway\_points": 0,

 "calibration\_factors": 3,

 "probe\_radius": 85,

 "mesh": {

 "x\_min": 15,

 "x\_max": 215,

 "y\_min": 15,

 "y\_max": 195,

 "radius": 85,

 "spacing": 20

 },

 "home\_first": false,

 "orthogonal": {

 "compensation": false,

 "height": 50,

 "deviations": [

 0,

 0,

 0

 ]

 },

 "network": {

 "enabled": true,

 "mac\_address": "",

 "name": "Ender 5 Upgrade #2",

 "password": "",

 "ssid": "",

 "ssid\_password": "",

 "dhcp": true,

 "ip": "192.168.1.20",

 "netmask": "255.255.255.0",

 "gateway": "192.168.1.254",

 "protocols": {

 "http": true,

 "ftp": false,

 "telnet": false

 }

 },

 "fans": [

 {

 "name": "",

 "value": 0,

 "inverted": false,

 "frequency": 500,

 "thermostatic": false,

 "heaters": [],

 "trigger\_temperature": 45,

 "output\_pin": "fan0"

 },

 {

 "name": "",

 "value": 100,

 "inverted": false,

 "frequency": 500,

 "thermostatic": true,

 "heaters": [

 1

 ],

 "trigger\_temperature": 45,

 "output\_pin": "fan1"

 },

 {

 "name": "",

 "value": 100,

 "inverted": false,

 "frequency": 500,

 "thermostatic": true,

 "heaters": [

 1,

 0

 ],

 "trigger\_temperature": 45,

 "output\_pin": "fan2"

 }

 ],

 "custom\_settings": "",

 "expansion\_boards": [],

 "standalone": true,

 "panelDue": true

}